
Pin modification:

P0.8 -> P0.6

P0.9 -> P0.7

Output (UART #2 ) explanation



State : the elevator’s current state


0 for fully closed

1 for opening

2 for fully opened

3 for closing

If the state of the door is changing



The current situation will also show

Floor : the current floor the elevator is



Direction : the direction of the elevator is going


0 for up

1 for down

Unfix bugs


1. sometimes IOSET1 didn’t set the value







Nothing happen

1. Even sometimes IOSET had successes set the port1 , sometimes measure fail to read the value and…







GPIO0 for midfloor never changes

一張含有 螢幕擷取畫面, 文字 的圖片

自動產生的描述